Strabo.core.exe (double X, Double Y, string WMSFolderPath, string TextRecognitionOutput, string LayerName)

(x1,Y1) (x2,y2)

(x3,y3) (x4,y4)

Input X means: x4 regarding the above image

Input Y means: Y1 regarding above image

WMSFolderPath: the path that WMS image will be saved in addition the output of binarization, text layer identification, color segmentation will be there, so this path is the input path of text detection step.

TextRecognitionOutput: where that output of text detection and Geojson output would be saved there.

LayerName: the layer that user want to crop a tile fro.